Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## G

getAction() - Method in class com.datecs.api.universalreader.TouchEvent
  Gets the kind of action being performed.
getBarcodeReader() - Method in class com.datecs.api.universalreader.UniversalReader
  Returns an instance of `BarcodeReader` class.
getBlocksSecurityStatus(int, int) - Method in class com.datecs.api.rfid.ISO15693Card
  Reads the security status of one more more blocks from ISO 15693 card.
getBytes() - Method in class com.datecs.api.smartcard.AnswerToReset
  Returns a copy of the bytes in this ATR.
getBytes() - Method in class com.datecs.api.smartcard.ResponseAPDU
  Returns a copy of the bytes in this APDU.
getCapabilities() - Method in class com.datecs.api.universalreader.UniversalReader
  Gets device capabilities.
getCaptureDeviceID() - Method in class com.datecs.api.biometric.AnsiIso
  Get capture device ID.
getCaptureDeviceIDAsHexString() - Method in class com.datecs.api.biometric.AnsiIso
  Get capture device ID as HEX String.
getChannel() - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Gets the channel number.
getChannel(int) - Method in class com.datecs.api.printer.ProtocolAdapter
  Gets an instance of `ProtocolAdapter.Channel` from specified channel number.
getCountOfViews() - Method in class com.datecs.api.biometric.AnsiIso
  Get count of views.
getData() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger image record data.
getData() - Method in class com.datecs.api.printer.PrinterInformation
  Returns a copy of the information data as returned from printer.
getData() - Method in class com.datecs.api.smartcard.AnswerToReset
  Returns a copy of the data bytes in the response body.
getData() - Method in class com.datecs.api.smartcard.ResponseAPDU
  Returns a copy of the data bytes in the response body.
getDataInputStream() - Method in interface com.datecs.api.hub.SerialPort
getDataOutputStream() - Method in interface com.datecs.api.hub.SerialPort
getElapse() - Method in class com.datecs.api.universalreader.TouchEvent
  Gets the time between this event and the previous one.
getErrorCode() - Method in exception com.datecs.api.biometric.TouchChipException
  Retrieves the exception error code for this instance.
getErrorCode() - Method in exception com.datecs.api.rfid.RFIDException
  Gets the error code that raise the exception.
getErrorCode() - Method in exception com.datecs.api.universalreader.UniversalReaderException
  Retrieves the exception error code for this instance.
getEvents() - Method in class com.datecs.api.universalreader.UniversalReader.TouchScreen
  Returns an instance of `TouchEvent[]`.
getExpiryMonth() - Method in class com.datecs.api.card.FinancialCard
  Returns an expiration month of this financial card.
getExpiryYear() - Method in class com.datecs.api.card.FinancialCard
  Returns an expiration year of this financial card.
getFeedLines() - Method in class com.datecs.api.printer.PrinterInformation
  Returns the number of dot lines needed to feed last printed line to cutter in.
getFingerDataBlockLength() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger data block length.
getFingerImageQuality() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger/palm image quality.
getFingerPosition() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger position.
getFirmwareVersion() - Method in class com.datecs.api.printer.PrinterInformation
  Returns the printer firmware version.
getFirmwareVersionString() - Method in class com.datecs.api.printer.PrinterInformation
  Returns the printer firmware version as string.
getFormatIdentifier() - Method in class com.datecs.api.biometric.AnsiIso
  Get format identifier.
getFormatIdentifierAsString() - Method in class com.datecs.api.biometric.AnsiIso
  Get format identifier as String.
getHeader() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger image record header data.
getHeaderAsHexString() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger image record header data as HEX string.
getHorizontalLineLength() - Method in class com.datecs.api.biometric.AnsiIso
  Get horizontal line length (image width).
getIdent() - Method in class com.datecs.api.hub.HUB
getIdentification() - Method in class com.datecs.api.universalreader.UniversalReader
  Gets the device identification string.
getIdentity(int, int, int, TouchChip.ImageReceiver) - Method in class com.datecs.api.biometric.TouchChip
  Gets a finger print data in different formats.
getIdentity() - Method in class com.datecs.api.biometric.TouchChip.Identity
  Get identity data.
getIdentityAsString() - Method in class com.datecs.api.biometric.TouchChip.Identity
  Get identity data.
getImageAsquisionLevel() - Method in class com.datecs.api.biometric.AnsiIso
  Get acquisition level.
getImageCompressionAlgorithm() - Method in class com.datecs.api.biometric.AnsiIso
  Get compression algorithm.
getImageData() - Method in class com.datecs.api.biometric.AnsiIso
  Get finger/palm image data.
getImageResolutionHorz() - Method in class com.datecs.api.biometric.AnsiIso
  Get image resolution (horizontal).
getImageResolutionVert() - Method in class com.datecs.api.biometric.AnsiIso
  Get image resolution (vertical).
getImpressionType() - Method in class com.datecs.api.biometric.AnsiIso
  Get impression type.
getInformation() - Method in class com.datecs.api.emsr.EMSR
  Returns information about encrypted magnetic stripe reader (EMSR).
getInformation() - Method in class com.datecs.api.printer.Printer
  Returns the printer information.
getInputStream() - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Gets the input stream from channel.
getKeyInformation(int) - Method in class com.datecs.api.emsr.EMSR
  Returns information about keys into encrypted magnetic stripe reader (EMSR).
getLastError() - Method in class com.datecs.api.rfid.RFID
  Get last error.
getLibraryInformation() - Method in class com.datecs.api.biometric.TouchChip
  Return TouchChip library information.
getMaxPageHeight() - Method in class com.datecs.api.printer.PrinterInformation
  Returns maximum page height in dots.
getMaxPageWidth() - Method in class com.datecs.api.printer.PrinterInformation
  Returns maximum page width in dots.
getMifareReader() - Method in class com.datecs.api.universalreader.UniversalReader
  Returns an instance of `MifareReader` class.
getModel() - Method in class com.datecs.api.hub.HUBIdent
getModel() - Method in class com.datecs.api.printer.PrinterInformation
  Return printer model.
getModule() - Method in class com.datecs.api.rfid.ContactlessCard
  Get RFID for this card.
getName() - Method in class com.datecs.api.card.FinancialCard
  Returns a card holder's name of this financial card.
getName() - Method in class com.datecs.api.hub.HUBIdent
getName() - Method in class com.datecs.api.printer.PrinterInformation
  Returns printer name.
getNumber() - Method in class com.datecs.api.card.FinancialCard
  Returns a unique identifier of this financial card.
getNumberOfFingers() - Method in class com.datecs.api.biometric.AnsiIso
  Get number of finger/palm.
getOutputStream() - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Gets the input stream from channel.
getPixelDepth() - Method in class com.datecs.api.biometric.AnsiIso
  Get pixel depth.
getPressure() - Method in class com.datecs.api.universalreader.TouchEvent
  Gets the current pressure of this event.
getProductIdentifier() - Method in class com.datecs.api.biometric.AnsiIso
  Get product identifier.
getProductIdentifierAsHexString() - Method in class com.datecs.api.biometric.AnsiIso
  Get product identifier as HEX string.
getProtocol() - Method in class com.datecs.api.smartcard.AnswerToReset
  Returns a smart card communication protocol.
getRawInputStream() - Method in class com.datecs.api.printer.ProtocolAdapter
  Get input stream that is not wrap by protocol data.
getRawOutputStream() - Method in class com.datecs.api.printer.ProtocolAdapter
  Get output stream that is not wrap by protocol data.
getRecordLength() - Method in class com.datecs.api.biometric.AnsiIso
  Get record length.
getScaleUnits() - Method in class com.datecs.api.biometric.AnsiIso
  Get scale units.
getScanResolutionHorz() - Method in class com.datecs.api.biometric.AnsiIso
  Get scan resolution (horizontal).
getScanResolutionVert() - Method in class com.datecs.api.biometric.AnsiIso
  Get scan resolution (vertical).
getSerialNumber() - Method in class com.datecs.api.universalreader.UniversalReader
  Gets the device serial number.
getSerialNumber() - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Gets the serial number of Mifare reader.
getSerialPort(int) - Method in class com.datecs.api.hub.HUB
getServiceCode() - Method in class com.datecs.api.card.FinancialCard
  Returns a service code.
getSettings(int) - Method in class com.datecs.api.printer.Printer
  Reading printer settings.
getSlot() - Method in class com.datecs.api.biometric.TouchChip.Identity
  Get identity slot.
getSmartCardReader() - Method in class com.datecs.api.universalreader.UniversalReader
  Returns an instance of `SmartCardReader` class.
getStatus() - Method in class com.datecs.api.printer.Printer
  Returns the printer status.
getStatus() - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Gets status data from channel.
getStatusCode() - Method in exception com.datecs.api.emsr.EMSRException
  Get status code that cause this exception.
getStatusCode() - Method in exception com.datecs.api.hub.HUBException
getSW() - Method in class com.datecs.api.smartcard.ResponseAPDU
  Returns the value of the status bytes SW1 and SW2 as a single status word SW.
getSW1() - Method in class com.datecs.api.smartcard.ResponseAPDU
  Returns the value of the status byte SW1 as a value between 0 and 255.
getSW2() - Method in class com.datecs.api.smartcard.ResponseAPDU
  Returns the value of the status byte SW2 as a value between 0 and 255.
getTemperature() - Method in class com.datecs.api.printer.Printer
  Returns the printer head temperature.
getTemplate(int) - Method in class com.datecs.api.biometric.TouchChip
  Get scanned template data.
getTemplate(int, int) - Method in class com.datecs.api.biometric.TouchChip
  Get template data from specific slot.
getTouchChip() - Method in class com.datecs.api.printer.Printer
  Get instance of TouchChip module.
getTouchScreen() - Method in class com.datecs.api.universalreader.UniversalReader
  Returns an instance of `Touchscreen` class.
getUID() - Method in class com.datecs.api.rfid.STSRICard
  Get UID.
getVersion() - Method in class com.datecs.api.hub.HUBIdent
getVersionNumber() - Method in class com.datecs.api.biometric.AnsiIso
  Get version number.
getVersionNumberAsString() - Method in class com.datecs.api.biometric.AnsiIso
  Get version number as String.
getVerticalLineLength() - Method in class com.datecs.api.biometric.AnsiIso
  Get vertical line length (image height).
getViewNumber() - Method in class com.datecs.api.biometric.AnsiIso
  Get view number.
getVoltage() - Method in class com.datecs.api.printer.Printer
  Returns the printer battery voltage.
getVoltagePercentage() - Method in class com.datecs.api.printer.Printer
  Returns the printer battery level in percents.
getX() - Method in class com.datecs.api.universalreader.TouchEvent
  Gets the X coordinate of this event.
getY() - Method in class com.datecs.api.universalreader.TouchEvent
  Gets the Y coordinate of this event.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W