Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## M

maxBlocks - Variable in class com.datecs.api.rfid.ContactlessCard
  The card max block size (Available for ISO15 cards only).
melody(String) - Method in class com.datecs.api.printer.Printer
  Making (beeping) a sequence of sounds with a certain frequency and duration.
MODE_READ_JIS - Static variable in class com.datecs.api.emsr.EMSR
  Read JIS card.
MODE_READ_PREFIX - Static variable in class com.datecs.api.emsr.EMSR
  Read data with prefix before tracks - 0xF0, 0xF1, 0xF2.
MODE_READ_RAW - Static variable in class com.datecs.api.emsr.EMSR
  Read raw data.
MODE_READ_TRACK1 - Static variable in class com.datecs.api.emsr.EMSR
  Read track 1.
MODE_READ_TRACK2 - Static variable in class com.datecs.api.emsr.EMSR
  Read track 2.
MODE_READ_TRACK3 - Static variable in class com.datecs.api.emsr.EMSR
  Read track 3.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W