Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## H

halt() - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Puts the selected Mifare card into 'idle' state.
HRI_ABOVE - Static variable in class com.datecs.api.printer.Printer
  The HRI code is drawn above the barcode.
HRI_BELOW - Static variable in class com.datecs.api.printer.Printer
  The HRI code is drawn below the barcode.
HRI_BOTH - Static variable in class com.datecs.api.printer.Printer
  The HRI code is drawn both above and below the barcode.
HRI_NONE - Static variable in class com.datecs.api.printer.Printer
  No HRI code is being drawn.
HUB - Class in com.datecs.api.hub
HUB(InputStream, OutputStream) - Constructor for class com.datecs.api.hub.HUB
HUB(FileDescriptor) - Constructor for class com.datecs.api.hub.HUB
HUBException - Exception in com.datecs.api.hub
HUBException(int) - Constructor for exception com.datecs.api.hub.HUBException
HUBIdent - Class in com.datecs.api.hub
hyatt64Card - Variable in class com.datecs.api.rfid.ContactlessCard
  The HYATT card enabled.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W