Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## I

IMAGE_COMPRESSION_NONE - Static variable in class com.datecs.api.biometric.TouchChip
  The image compression type.
IMAGE_FORMAT_ANSI - Static variable in class com.datecs.api.biometric.TouchChip
  The image is in ANSI format.
IMAGE_FORMAT_ISO - Static variable in class com.datecs.api.biometric.TouchChip
  The image is in ISO format.
IMAGE_SIZE_LARGE - Static variable in class com.datecs.api.biometric.TouchChip
  The image size is 256x360 pixels.
IMAGE_SIZE_SMALL - Static variable in class com.datecs.api.biometric.TouchChip
  The image size is 192x270 pixels.
increment(int, int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Performs value increment operation in Mifare card.
initialize() - Method in class com.datecs.api.rfid.FeliCaCard
  Initialize card.
initialize() - Method in class com.datecs.api.rfid.ISO14443Card
  Initialize card.
initialize() - Method in class com.datecs.api.rfid.ISO15693Card
  Initialize card.
initialize() - Method in class com.datecs.api.rfid.STSRICard
  Initialize card.
isActive() - Method in interface com.datecs.api.hub.SerialPort
isBarcodeAvailable() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if barcode reader module is available.
isBlackmarkEnabled() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if blackmark mode is enabled.
isBlackmarkSupported() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if blackmark mode is supported.
isButtonPressed() - Method in class com.datecs.api.universalreader.UniversalReader
  Gets the current state of the button.
isButtonPressed(boolean) - Method in class com.datecs.api.universalreader.UniversalReader
  Gets the current state of the button.
isCardPresent() - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Returns if smart card is present into reader.
isFahrenheit() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if head temperature is returned in Fahrenheit scale.
isFirmwareUpdateSupported() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if printer support firmware update.
isIrdaAvailable() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if IRDA module is available.
isMsr3Tack() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if magnetic stripe reader is capable to read track 3.
isMsrAvailable() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if magnetic stripe reader module is available.
ISO14443Card - Class in com.datecs.api.rfid
  A class that represents ISO14443 cards.
ISO14443Card(RC663) - Constructor for class com.datecs.api.rfid.ISO14443Card
  Constructs a new instance of this class.
ISO15693Card - Class in com.datecs.api.rfid
  A class that represents ISO15693 cards.
ISO15693Card(RC663) - Constructor for class com.datecs.api.rfid.ISO15693Card
  Constructs a new instance of this class.
isPageSupported() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if page mode is supported.
isProtocolEnabled() - Method in class com.datecs.api.printer.ProtocolAdapter
  Return `true` if protocol mode is currently enabled.
isUsbAEnabled() - Method in class com.datecs.api.printer.PrinterInformation
  Return `true` if USB A is enabled.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W