Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

# Constant Field Values

Contents

- com.datecs.*

com.datecs.*

com.datecs.api.BuildInfo
`public static final java.lang.String` | `VERSION` | `"3.5.84"`

com.datecs.api.biometric.TouchChip
`public static final int` | `IMAGE_COMPRESSION_NONE` | `0`
`public static final int` | `IMAGE_FORMAT_ANSI` | `0`
`public static final int` | `IMAGE_FORMAT_ISO` | `1`
`public static final int` | `IMAGE_SIZE_LARGE` | `1`
`public static final int` | `IMAGE_SIZE_SMALL` | `0`
`public static final int` | `TEMPLATE_FORMAT_ANSI` | `1`
`public static final int` | `TEMPLATE_FORMAT_ISO_FMC_C` | `4`
`public static final int` | `TEMPLATE_FORMAT_ISO_FMC_N` | `3`
`public static final int` | `TEMPLATE_FORMAT_ISO_FMR` | `2`
`public static final int` | `TEMPLATE_FORMAT_NATIVE` | `0`

com.datecs.api.emsr.EMSR
`public static final int` | `ENCRYPTION_TYPE_AES256` | `2`
`public static final int` | `ENCRYPTION_TYPE_IDTECH` | `3`
`public static final int` | `ENCRYPTION_TYPE_OLD_RSA` | `0`
`public static final int` | `ENCRYPTION_TYPE_RSA` | `5`
`public static final int` | `KEY_AES_AUTHENTICATION` | `0`
`public static final int` | `KEY_AES_DATA_ENCRYPTION` | `1`
`public static final int` | `KEY_AES_KEK` | `2`
`public static final int` | `KEY_DUKPT_MASTER` | `32`
`public static final int` | `KEY_NO_KEY` | `255`
`public static final int` | `KEY_TMK_AES` | `16`
`public static final int` | `MODE_READ_JIS` | `32`
`public static final int` | `MODE_READ_PREFIX` | `128`
`public static final int` | `MODE_READ_RAW` | `64`
`public static final int` | `MODE_READ_TRACK1` | `1`
`public static final int` | `MODE_READ_TRACK2` | `2`
`public static final int` | `MODE_READ_TRACK3` | `4`
`public static final int` | `STATUS_EMSR_BAD_ARRAY` | `16`
`public static final int` | `STATUS_EMSR_BARCODE_MISHMASH` | `18`
`public static final int` | `STATUS_EMSR_BARCODE_NO_READER` | `19`
`public static final int` | `STATUS_EMSR_CARD_ERROR` | `3`
`public static final int` | `STATUS_EMSR_HARD` | `23`
`public static final int` | `STATUS_EMSR_INVALID_COMMAND` | `1`
`public static final int` | `STATUS_EMSR_INVALID_LENGTH` | `20`
`public static final int` | `STATUS_EMSR_INVALID_SIGNATURE` | `22`
`public static final int` | `STATUS_EMSR_NO_BARCODE_READ` | `17`
`public static final int` | `STATUS_EMSR_NO_DATA` | `6`
`public static final int` | `STATUS_EMSR_NO_PERMITION` | `2`
`public static final int` | `STATUS_EMSR_NO_RESPONSE` | `5`
`public static final int` | `STATUS_EMSR_SYNTAX_ERROR` | `4`
`public static final int` | `STATUS_EMSR_TAMPERED` | `21`

com.datecs.api.hub.HUB
`public static final int` | `EVENT_NONE` | `0`
`public static final int` | `EVENT_SERIAL_PORT_RECV` | `1`
`public static final int` | `EVENT_USB_RECV` | `2`
`public static final int` | `SERIAL_PORT_1` | `0`
`public static final int` | `SERIAL_PORT_2` | `1`
`public static final int` | `SERIAL_PORT_3` | `2`
`public static final int` | `STATUS_INVALID_COMMAND` | `3`
`public static final int` | `STATUS_INVALID_PARAMETER` | `5`
`public static final int` | `STATUS_NO_DATA` | `2`
`public static final int` | `STATUS_NO_RESPONSE` | `1`
`public static final int` | `STATUS_OK` | `0`
`public static final int` | `STATUS_SYNTAX_ERROR` | `4`

com.datecs.api.printer.Printer
`public static final int` | `ALIGN_CENTER` | `1`
`public static final int` | `ALIGN_LEFT` | `0`
`public static final int` | `ALIGN_RIGHT` | `2`
`public static final int` | `BARCODE_CODABAR` | `71`
`public static final int` | `BARCODE_CODE128` | `73`
`public static final int` | `BARCODE_CODE128AUTO` | `75`
`public static final int` | `BARCODE_CODE39` | `69`
`public static final int` | `BARCODE_CODE93` | `72`
`public static final int` | `BARCODE_EAN128` | `76`
`public static final int` | `BARCODE_EAN13` | `67`
`public static final int` | `BARCODE_EAN8` | `68`
`public static final int` | `BARCODE_ITF` | `70`
`public static final int` | `BARCODE_PDF417` | `74`
`public static final int` | `BARCODE_UPCA` | `65`
`public static final int` | `BARCODE_UPCE` | `66`
`public static final int` | `FILL_BLACK` | `1`
`public static final int` | `FILL_INVERTED` | `2`
`public static final int` | `FILL_WHITE` | `0`
`public static final int` | `HRI_ABOVE` | `1`
`public static final int` | `HRI_BELOW` | `2`
`public static final int` | `HRI_BOTH` | `3`
`public static final int` | `HRI_NONE` | `0`
`public static final int` | `PAGE_BOTTOM` | `1`
`public static final int` | `PAGE_LEFT` | `0`
`public static final int` | `PAGE_RIGHT` | `2`
`public static final int` | `PAGE_TOP` | `3`
`public static final int` | `SETTINGS_BLUETOOTH` | `5`

com.datecs.api.printer.PrinterInformation
`public static final int` | `PRINTER_CMP10` | `0`
`public static final int` | `PRINTER_DPP250` | `2`
`public static final int` | `PRINTER_DPP350` | `1`
`public static final int` | `PRINTER_DPP450` | `5`
`public static final int` | `PRINTER_DPP500` | `8`
`public static final int` | `PRINTER_EP300` | `7`
`public static final int` | `PRINTER_EP55` | `4`
`public static final int` | `PRINTER_EP60` | `6`
`public static final int` | `PRINTER_PP60` | `3`
`public static final int` | `PRINTER_UNKNOWN` | `-1`

com.datecs.api.printer.ProtocolAdapter
`public static final int` | `CHANNEL_EMSR` | `15`
`public static final int` | `CHANNEL_PRINTER` | `1`
`public static final int` | `CHANNEL_RFID` | `13`
`public static final int` | `CHANNEL_UNIVERSAL_READER` | `16`

com.datecs.api.rfid.ContactlessCard
`public static final int` | `CARD_FELICA` | `11`
`public static final int` | `CARD_ISO14443A` | `6`
`public static final int` | `CARD_ISO14443B` | `10`
`public static final int` | `CARD_ISO15693` | `8`
`public static final int` | `CARD_MIFARE_CLASSIC_1K` | `2`
`public static final int` | `CARD_MIFARE_CLASSIC_4K` | `3`
`public static final int` | `CARD_MIFARE_DESFIRE` | `9`
`public static final int` | `CARD_MIFARE_MINI` | `1`
`public static final int` | `CARD_MIFARE_PLUS` | `7`
`public static final int` | `CARD_MIFARE_ULTRALIGHT` | `4`
`public static final int` | `CARD_MIFARE_ULTRALIGHT_C` | `5`
`public static final int` | `CARD_ST_SRI` | `12`
`public static final int` | `CARD_UNKNOWN` | `0`

com.datecs.api.rfid.FeliCaCard
`public static final int` | `FELICA_SMARTTAG_BATTERY_LOW1` | `2`
`public static final int` | `FELICA_SMARTTAG_BATTERY_LOW2` | `3`
`public static final int` | `FELICA_SMARTTAG_BATTERY_NORMAL1` | `0`
`public static final int` | `FELICA_SMARTTAG_BATTERY_NORMAL2` | `1`
`public static final int` | `FELICA_SMARTTAG_DRAW_BLACK_BACKGROUND` | `1`
`public static final int` | `FELICA_SMARTTAG_DRAW_KEEP_BACKGROUND` | `2`
`public static final int` | `FELICA_SMARTTAG_DRAW_USE_LAYOUT` | `3`
`public static final int` | `FELICA_SMARTTAG_DRAW_WHITE_BACKGROUND` | `0`

com.datecs.api.rfid.RC663
`public static final int` | `CHANNEL_FELICA` | `4`
`public static final int` | `CHANNEL_ISO1443A` | `1`
`public static final int` | `CHANNEL_ISO1443B` | `2`
`public static final int` | `CHANNEL_ISO15693` | `3`
`public static final int` | `CHANNEL_MAIN` | `0`
`public static final int` | `CHANNEL_STSRI` | `5`

com.datecs.api.rfid.RFID
`public static final int` | `CARD_SUPPORT_FELICA` | `4`
`public static final int` | `CARD_SUPPORT_ISO15` | `32`
`public static final int` | `CARD_SUPPORT_JEWEL` | `16`
`public static final int` | `CARD_SUPPORT_NFC` | `8`
`public static final int` | `CARD_SUPPORT_STSRI` | `64`
`public static final int` | `CARD_SUPPORT_TYPE_A` | `1`
`public static final int` | `CARD_SUPPORT_TYPE_B` | `2`

com.datecs.api.rfid.RFIDException
`public static final int` | `ERROR_FAILED` | `-20`
`public static final int` | `ERROR_MIFARE_EACCESS` | `-10013`
`public static final int` | `ERROR_MIFARE_EAUTHENTICATION` | `-10010`
`public static final int` | `ERROR_MIFARE_EBASE` | `-10000`
`public static final int` | `ERROR_MIFARE_EBIT` | `-10012`
`public static final int` | `ERROR_MIFARE_ECODE` | `-10011`
`public static final int` | `ERROR_MIFARE_ECOLLISION` | `-10002`
`public static final int` | `ERROR_MIFARE_ECRC` | `-10005`
`public static final int` | `ERROR_MIFARE_EEEPROM` | `-10007`
`public static final int` | `ERROR_MIFARE_EFIFO` | `-10006`
`public static final int` | `ERROR_MIFARE_EFRAME` | `-10004`
`public static final int` | `ERROR_MIFARE_EGENERIC` | `-10009`
`public static final int` | `ERROR_MIFARE_EKEY` | `-10008`
`public static final int` | `ERROR_MIFARE_EPARITY` | `-10003`
`public static final int` | `ERROR_MIFARE_ETIMEOUT` | `-10001`
`public static final int` | `ERROR_MIFARE_EVALUE` | `-10014`
`public static final int` | `ERROR_TIMEOUT` | `-6`

com.datecs.api.smartcard.AnswerToReset
`public static final int` | `PROTOCOL_T0` | `0`
`public static final int` | `PROTOCOL_T1` | `1`

com.datecs.api.universalreader.TouchEvent
`public static final int` | `ACTION_DOWN` | `0`
`public static final int` | `ACTION_UP` | `1`

com.datecs.api.universalreader.UniversalReader
`public static final int` | `BUTTON_MODE_BARCODE` | `1`
`public static final int` | `BUTTON_MODE_NONE` | `0`
`public static final int` | `BUTTON_MODE_STATUS` | `2`
`public static final int` | `CAPABILITY_BARCODE` | `4`
`public static final int` | `CAPABILITY_BUTTON` | `64`
`public static final int` | `CAPABILITY_DEBUG` | `1`
`public static final int` | `CAPABILITY_EV15` | `1024`
`public static final int` | `CAPABILITY_FIRMWARE` | `256`
`public static final int` | `CAPABILITY_GSM` | `16`
`public static final int` | `CAPABILITY_LCD2X16` | `128`
`public static final int` | `CAPABILITY_MAGNETIC` | `512`
`public static final int` | `CAPABILITY_MIFARE` | `32`
`public static final int` | `CAPABILITY_SMARTCARD` | `2`
`public static final int` | `CAPABILITY_TOUCHSCREEN` | `8`
`public static final int` | `ERROR_0K` | `0`
`public static final int` | `ERROR_BARCODE` | `16`
`public static final int` | `ERROR_BARCODE_INVALID` | `18`
`public static final int` | `ERROR_BARCODE_NODATA` | `17`
`public static final int` | `ERROR_BARCODE_NOTPRESENT` | `19`
`public static final int` | `ERROR_CARD` | `3`
`public static final int` | `ERROR_INVALID` | `1`
`public static final int` | `ERROR_MIFARE_ACCESS` | `-13`
`public static final int` | `ERROR_MIFARE_AUTHENTICATION` | `-10`
`public static final int` | `ERROR_MIFARE_BIT` | `-12`
`public static final int` | `ERROR_MIFARE_CODE` | `-11`
`public static final int` | `ERROR_MIFARE_COLLISION` | `-2`
`public static final int` | `ERROR_MIFARE_CRC` | `-5`
`public static final int` | `ERROR_MIFARE_EEPROM` | `-7`
`public static final int` | `ERROR_MIFARE_FIFO` | `-6`
`public static final int` | `ERROR_MIFARE_FRAME` | `-4`
`public static final int` | `ERROR_MIFARE_GENERIC` | `-9`
`public static final int` | `ERROR_MIFARE_KEY` | `-8`
`public static final int` | `ERROR_MIFARE_PARITY` | `-3`
`public static final int` | `ERROR_MIFARE_TIMEOUT` | `-1`
`public static final int` | `ERROR_MIFARE_VALUE` | `-14`
`public static final int` | `ERROR_NODATA` | `6`
`public static final int` | `ERROR_NORESPONCE` | `5`
`public static final int` | `ERROR_NOTPERMITTED` | `2`
`public static final int` | `ERROR_SYNTAX` | `4`

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES