Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## D

decrement(int, int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Performs value decrement operation in Mifare card.
deleteIdentity(int) - Method in class com.datecs.api.biometric.TouchChip
  Delete an already enrolled template at a specified slot in the TouchChip module non-volatile memory.
disable() - Method in class com.datecs.api.emsr.EMSR
  Disable encrypted magnetic stripe reader (EMSR).
disable() - Method in class com.datecs.api.rfid.RC663
  Powers on the RF card reader module and release associated resources.
displayText(String, String) - Method in class com.datecs.api.universalreader.UniversalReader
  Display text.
drawPageFrame(int, int, int, int, int, int) - Method in class com.datecs.api.printer.Printer
  Draws a rectangle frame with selected thickness in page mode.
drawPageRectangle(int, int, int, int, int) - Method in class com.datecs.api.printer.Printer
  Draws a rectangle in page mode.
dsfid - Variable in class com.datecs.api.rfid.ContactlessCard
  The card data storage format identifier (Available for ISO15 cards only).

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W