Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## A

ACTION_DOWN - Static variable in class com.datecs.api.universalreader.TouchEvent
  A pressed gesture has started, the touch event contains a valid location of event.
ACTION_UP - Static variable in class com.datecs.api.universalreader.TouchEvent
  A pressed gesture has finished, the touch event does not contains a valid location.
afi - Variable in class com.datecs.api.rfid.ContactlessCard
  The card AFI (Available for ISO15 cards only).
ALIGN_CENTER - Static variable in class com.datecs.api.printer.Printer
  The printing object is centered.
ALIGN_LEFT - Static variable in class com.datecs.api.printer.Printer
  The printing object is left aligned.
ALIGN_RIGHT - Static variable in class com.datecs.api.printer.Printer
  The printing object is left aligned.
AnsiIso - Class in com.datecs.api.biometric
  Finger Image-Based Data Interchange Format parser.
AnswerToReset - Class in com.datecs.api.smartcard
  This class represents the smart card response ATR as defined in ISO/IEC 7816-4.
AnswerToReset(byte[]) - Constructor for class com.datecs.api.smartcard.AnswerToReset
  Constructs a new instance of this class from a given byte array.
anticollision() - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Returns the serial number of one of requested Mifare cards.
atqa - Variable in class com.datecs.api.rfid.ContactlessCard
  The card ATQA (Available for MIFARE cards only).
authenticate(char, int, byte[]) - Method in class com.datecs.api.rfid.ISO14443Card
  Authenticate mifare card block with direct key data.
authenticate(char, int, int) - Method in class com.datecs.api.rfid.ISO14443Card
  Authenticate mifare card block with previously stored key.
authenticate(int, int, int, byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Authenticates Mifare card for operation.
authenticate(int, int, int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Authenticates Mifare card for operation with key stored into Mifare reader EEPROM memory.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W