Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## S

sak - Variable in class com.datecs.api.rfid.ContactlessCard
  The card SAK (Available for MIFARE cards only).
select(int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Selects a Mifare card.
select(int) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Selects the smart card reader slot.
selectCodetable(int) - Method in class com.datecs.api.printer.Printer
  Selects a code table.
selectPageMode() - Method in class com.datecs.api.printer.Printer
  Switches from standard mode to page mode.
selectStandardMode() - Method in class com.datecs.api.printer.Printer
  Switches from page mode to standard mode.
serial - Variable in class com.datecs.api.emsr.EMSR.EMSRInformation
  Device serial number
SERIAL_PORT_1 - Static variable in class com.datecs.api.hub.HUB
SERIAL_PORT_2 - Static variable in class com.datecs.api.hub.HUB
SERIAL_PORT_3 - Static variable in class com.datecs.api.hub.HUB
SerialPort - Interface in com.datecs.api.hub
setAlign(int) - Method in class com.datecs.api.printer.Printer
  Sets alignment for the next printed text row or object.
setAutoOff(int) - Method in class com.datecs.api.universalreader.UniversalReader
  Set auto off time.
setBarcode(int, boolean, int, int, int) - Method in class com.datecs.api.printer.Printer
  Sets the various barcode parameters.
setBarcodeListener(ProtocolAdapter.BarcodeListener) - Method in class com.datecs.api.printer.ProtocolAdapter
  Set a callback listener to notify for barcode event.
setBarcodeListener(UniversalReader.BarcodeListener) - Method in class com.datecs.api.universalreader.UniversalReader
  Set a callback listener to notify for barcode event.
setButton(int) - Method in class com.datecs.api.universalreader.UniversalReader
  Set button function mode
setButtonListener(UniversalReader.ButtonListener) - Method in class com.datecs.api.universalreader.UniversalReader
  Set a callback listener to notify for button state changed.
setCardListener(ProtocolAdapter.CardListener) - Method in class com.datecs.api.printer.ProtocolAdapter
  Set a callback listener to notify for card event.
setCardListener(RC663.CardListener) - Method in class com.datecs.api.rfid.RC663
  Set a callback to notify when new card available.
setCardListener(UniversalReader.CardListener) - Method in class com.datecs.api.universalreader.UniversalReader
  Set a callback listener to notify for card event.
setChannel(int, int) - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Sets channel associated port.
setConfig(int, int, int) - Method in interface com.datecs.api.hub.SerialPort
setConnectionListener(Printer.ConnectionListener) - Method in class com.datecs.api.printer.Printer
  Set a callback listener to notify the connection state is changed.
setConnectionListener(UniversalReader.ConnectionListener) - Method in class com.datecs.api.universalreader.UniversalReader
  Set a callback listener to notify the connection state is changed.
setDebug(boolean) - Static method in class com.datecs.api.emsr.EMSR
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.api.printer.Printer
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.api.printer.ProtocolAdapter
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.api.universalreader.UniversalReader
  Specify whether the object can output debug information
setEncryptionType(int) - Method in class com.datecs.api.emsr.EMSR
  Set encryption type.
setFlowControl(int) - Method in interface com.datecs.api.hub.SerialPort
setIntensity(int) - Method in class com.datecs.api.printer.Printer
  Set intensity level.
setLedMode(int) - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Set LED indicator mode.
setLineSpace(int) - Method in class com.datecs.api.printer.Printer
  Sets the line space of text rows.
setPageRegion(int, int, int, int, int) - Method in class com.datecs.api.printer.Printer
  Defines the relative position, size print direction of the page.
setPageXY(int, int) - Method in class com.datecs.api.printer.Printer
  Sets the print position in current page region.
setPower(boolean) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Powers on/off Mifare card reader.
setPower(boolean) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Powers on/off smart card.
setPrinterListener(ProtocolAdapter.PrinterListener) - Method in class com.datecs.api.printer.ProtocolAdapter
  Set a callback listener to notify for printer event.
setTemplate(int, byte[]) - Method in class com.datecs.api.biometric.TouchChip
  Set template data to into TouchChip module non-volatile memory.
SETTINGS_BLUETOOTH - Static variable in class com.datecs.api.printer.Printer
  Bluetooth settings.
smartTagClearScreen() - Method in class com.datecs.api.rfid.FeliCaCard
  Clears the screen of FeliCa SmartTag.
smartTagDisplayLayout(int) - Method in class com.datecs.api.rfid.FeliCaCard
  Displays previously stored layout.
smartTagDrawImage(int, int, int, int, int, int, byte[]) - Method in class com.datecs.api.rfid.FeliCaCard
  Draws image on FeliCa SmartTag's screen.
smartTagGetBatteryStatus() - Method in class com.datecs.api.rfid.FeliCaCard
  Returns FeliCa SmartTag battery status.
smartTagRead(int, int) - Method in class com.datecs.api.rfid.FeliCaCard
  Writes data in FeliCa SmartTag.
smartTagSaveLayout(int) - Method in class com.datecs.api.rfid.FeliCaCard
  Saves the current display as layout number.
smartTagWrite(int, byte[]) - Method in class com.datecs.api.rfid.FeliCaCard
  Writes data in FeliCa SmartTag.
STATUS_EMSR_BAD_ARRAY - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_BARCODE_MISHMASH - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_BARCODE_NO_READER - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_CARD_ERROR - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_HARD - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_INVALID_COMMAND - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_INVALID_LENGTH - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_INVALID_SIGNATURE - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_NO_BARCODE_READ - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_NO_DATA - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_NO_PERMITION - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_NO_RESPONSE - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_SYNTAX_ERROR - Static variable in class com.datecs.api.emsr.EMSR
STATUS_EMSR_TAMPERED - Static variable in class com.datecs.api.emsr.EMSR
STATUS_INVALID_COMMAND - Static variable in class com.datecs.api.hub.HUB
STATUS_INVALID_PARAMETER - Static variable in class com.datecs.api.hub.HUB
STATUS_NO_DATA - Static variable in class com.datecs.api.hub.HUB
STATUS_NO_RESPONSE - Static variable in class com.datecs.api.hub.HUB
STATUS_OK - Static variable in class com.datecs.api.hub.HUB
STATUS_SYNTAX_ERROR - Static variable in class com.datecs.api.hub.HUB
STSRICard - Class in com.datecs.api.rfid
STSRICard(RC663) - Constructor for class com.datecs.api.rfid.STSRICard
  Constructs a new instance of this class.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W