Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## W

waitRemove() - Method in class com.datecs.api.rfid.ContactlessCard
  Call this function once you are done with the card.
wipeIdentity() - Method in class com.datecs.api.biometric.TouchChip
  Wipe identity content.
write(int) - Method in class com.datecs.api.printer.Printer
  Writes the specified byte to this printer.
write(byte[]) - Method in class com.datecs.api.printer.Printer
  Writes all bytes from the specified byte array to this printer.
write(byte[], int, int) - Method in class com.datecs.api.printer.Printer
  Writes `length` bytes from the specified byte array to this printer.
write(int, int, byte[]) - Method in class com.datecs.api.rfid.FeliCaCard
  Writes one more more blocks of data to FeliCa card.
write(int, byte[]) - Method in class com.datecs.api.rfid.ISO15693Card
  Writes one more more blocks of data to ISO 15693 card.
write(int, byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Writes block to Mifare card.
write(int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Writes data to Mifare card.
write(int, int, int, int, byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Sends APDU write request.
write(byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Sends APDU write request.
write16(int, byte[]) - Method in class com.datecs.api.rfid.ISO14443Card
  Writes one block of data to Mifare Classic/Ultralight cards.
writeAFI(byte) - Method in class com.datecs.api.rfid.ISO15693Card
  Changes ISO 15693 card AFI.
writeBlock(int, byte[]) - Method in class com.datecs.api.rfid.STSRICard
  Writes one more more blocks of data to ST SRI card.
writeDSFID(byte) - Method in class com.datecs.api.rfid.ISO15693Card
  Changes ISO 15693 card DSFID.
writeEeprom(int, byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Writes data to Mifare reader EEPROM memory.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W