Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
com.datecs.api.rfid.RFIDException

Packages that use RFIDException
com.datecs.api.rfid |

Uses of RFIDException in com.datecs.api.rfid

Methods in com.datecs.api.rfid that throw RFIDException
`void` | `ISO14443Card.authenticate(char type, int address, byte[] key)` Authenticate mifare card block with direct key data.
`void` | `ISO14443Card.authenticate(char type, int address, int keyIndex)` Authenticate mifare card block with previously stored key.
`void` | `STSRICard.completion()` Card completion.
`void` | `RC663.disable()` Powers on the RF card reader module and release associated resources.
`void` | `RC663.enable()` Initializes and powers on the RF card reader module.
`byte[]` | `ISO15693Card.getBlocksSecurityStatus(int startBlock, int blocks)` Reads the security status of one more more blocks from ISO 15693 card.
`byte[]` | `STSRICard.getUID()` Get UID.
`void` | `ISO14443Card.loadKey(int keyIndex, char type, byte[] key)` Store key in the internal module memory for later use.
`void` | `ISO15693Card.lockAFI()` Locks ISO 15693 AFI preventing further changes.
`void` | `ISO15693Card.lockBlock(int block)` Locks a single ISO 15693 card block.
`void` | `ISO15693Card.lockDSFID()` Locks ISO 15693 card DSFID preventing further changes.
`byte[]` | `ISO15693Card.read(int startBlock, int blocks)` Reads one more more blocks of data from ISO 15693 card.
`byte[]` | `FeliCaCard.read(int serviceCode, int startBlock, int blocks)` Reads one more more blocks of data from FeliCa card.
`byte[]` | `ISO14443Card.read16(int address)` Reads one block of data from Mifare Classic/Ultralight cards.
`byte[]` | `STSRICard.readBlock(int address)` Reads one more more blocks of data from ST SRI card.
`void` | `STSRICard.reset()` Card reset.
`void` | `RC663.resume()` Reinitialize RF card reader module to listen for cards.
`void` | `FeliCaCard.smartTagClearScreen()` Clears the screen of FeliCa SmartTag.
`void` | `FeliCaCard.smartTagDisplayLayout(int layout)` Displays previously stored layout.
`void` | `FeliCaCard.smartTagDrawImage(int x, int y, int width, int height, int drawMode, int layout, byte[] data)` Draws image on FeliCa SmartTag's screen.
`int` | `FeliCaCard.smartTagGetBatteryStatus()` Returns FeliCa SmartTag battery status.
`byte[]` | `FeliCaCard.smartTagRead(int address, int length)` Writes data in FeliCa SmartTag.
`void` | `FeliCaCard.smartTagSaveLayout(int layout)` Saves the current display as layout number.
`void` | `FeliCaCard.smartTagWrite(int address, byte[] data)` Writes data in FeliCa SmartTag.
`byte[]` | `RC663.transmitCard(int channel, byte[] data)` Transmit command data to card.
`byte[]` | `RC663.transmitCard(int channel, byte[] data, int length)` Transmit command data to card.
`void` | `ISO14443Card.ulcAuthenticate(byte[] key)` Performs 3DES authentication of Mifare Ultralight C card using the given key.
`void` | `ISO14443Card.ulcSetKey(byte[] key)` Sets the 3DES key of Mifare Ultralight C cards.
`int` | `ISO15693Card.write(int startBlock, byte[] data)` Writes one more more blocks of data to ISO 15693 card.
`void` | `FeliCaCard.write(int serviceCode, int startBlock, byte[] data)` Writes one more more blocks of data to FeliCa card.
`void` | `ISO14443Card.write16(int address, byte[] data)` Writes one block of data to Mifare Classic/Ultralight cards.
`void` | `ISO15693Card.writeAFI(byte afi)` Changes ISO 15693 card AFI.
`void` | `STSRICard.writeBlock(int address, byte[] data)` Writes one more more blocks of data to ST SRI card.
`void` | `ISO15693Card.writeDSFID(byte dsfid)` Changes ISO 15693 card DSFID.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES