Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## R

RC663 - Class in com.datecs.api.rfid
  This class represents RC663 module.
RC663(InputStream, OutputStream, int) - Constructor for class com.datecs.api.rfid.RC663
  Constructs a new instance of this class.
RC663(InputStream, OutputStream) - Constructor for class com.datecs.api.rfid.RC663
  Constructs a new instance of this class.
RC663.CardListener - Interface in com.datecs.api.rfid
read(int, int, int) - Method in class com.datecs.api.rfid.FeliCaCard
  Reads one more more blocks of data from FeliCa card.
read(int, int) - Method in class com.datecs.api.rfid.ISO15693Card
  Reads one more more blocks of data from ISO 15693 card.
read() - Method in class com.datecs.api.universalreader.UniversalReader.BarcodeReader
  Reads barcode.
read(int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Reads block from Mifare card.
read(int, int, int, int, int) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Sends APDU read request.
read(byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Sends APDU read request.
read16(int) - Method in class com.datecs.api.rfid.ISO14443Card
  Reads one block of data from Mifare Classic/Ultralight cards.
readBarcode(int) - Method in class com.datecs.api.printer.Printer
  Reads the barcode.
readBlock(int) - Method in class com.datecs.api.rfid.STSRICard
  Reads one more more blocks of data from ST SRI card.
readCard(boolean, boolean, boolean, int) - Method in class com.datecs.api.printer.Printer
  Reads the magnetic stripe card.
readCardData(int) - Method in class com.datecs.api.emsr.EMSR
  Read card data.
readEeprom(int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Reads data from Mifare reader EEPROM memory.
readTrackData(int) - Method in class com.datecs.api.universalreader.UniversalReader
  Read track data.
request(boolean) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Requests for Mifare cards.
reset() - Method in class com.datecs.api.printer.Printer
  Resets printer to it's default settings.
reset() - Method in class com.datecs.api.rfid.STSRICard
  Card reset.
reset() - Method in class com.datecs.api.universalreader.UniversalReader.SmartCardReader
  Resets the smart card and returns the ATR.
ResponseAPDU - Class in com.datecs.api.smartcard
  This class represents the smart card response APDU as defined in ISO/IEC 7816-4.
ResponseAPDU(byte[]) - Constructor for class com.datecs.api.smartcard.ResponseAPDU
  Constructs a new instance of this class from a given byte array containing the complete APDU contents.
restore(int, int, int) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Performs value restore operation in Mifare card.
resume() - Method in class com.datecs.api.rfid.RC663
  Reinitialize RF card reader module to listen for cards.
RFID - Class in com.datecs.api.rfid
  Class that represents RFID module.
RFIDException - Exception in com.datecs.api.rfid
  The exception that is thrown when an RC663 module error occurs.
RFIDException(int) - Constructor for exception com.datecs.api.rfid.RFIDException
  Initializes a new instance of the RC663Exception class with its error code.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W