Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## L

listSlots() - Method in class com.datecs.api.biometric.TouchChip
  Lists all slots in which there is an enrolled template.
loadKey(byte[]) - Method in class com.datecs.api.emsr.EMSR
  Loads new key, in plain or encrypted with already loaded AES256 Key Encryption Key (KEK).
loadKey(int, char, byte[]) - Method in class com.datecs.api.rfid.ISO14443Card
  Store key in the internal module memory for later use.
loadKey(int, byte[]) - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Stores key into Mifare reader EEPROM.
lockAFI() - Method in class com.datecs.api.rfid.ISO15693Card
  Locks ISO 15693 AFI preventing further changes.
lockBlock(int) - Method in class com.datecs.api.rfid.ISO15693Card
  Locks a single ISO 15693 card block.
lockDSFID() - Method in class com.datecs.api.rfid.ISO15693Card
  Locks ISO 15693 card DSFID preventing further changes.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W