Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## E

EMSR - Class in com.datecs.api.emsr
EMSR(InputStream, OutputStream) - Constructor for class com.datecs.api.emsr.EMSR
  Constructs a new instance of this class from a given `InputStream` and `OutputStream`.
EMSR.EMSRInformation - Class in com.datecs.api.emsr
  The class that contains various information about encrypted magnetic stripe reader (EMSR).
EMSR.EMSRKeyInformation - Class in com.datecs.api.emsr
  The class that contains various information about encrypted magnetic stripe reader (EMSR).
EMSRException - Exception in com.datecs.api.emsr
  Encrypted magnetic stripe reader exception class.
EMSRException(int) - Constructor for exception com.datecs.api.emsr.EMSRException
  Create a new instance of `EMSRException` class.
enable() - Method in class com.datecs.api.emsr.EMSR
  Enable encrypted magnetic stripe reader (EMSR).
enable() - Method in class com.datecs.api.rfid.RC663
  Initializes and powers on the RF card reader module.
enableMagneticCardReader(boolean) - Method in class com.datecs.api.universalreader.UniversalReader
  Enables magnetic card reader.
enableMagneticCardReaderEvents(boolean) - Method in class com.datecs.api.universalreader.UniversalReader
ENCRYPTION_TYPE_AES256 - Static variable in class com.datecs.api.emsr.EMSR
  Encrypted Magnetic Head AES 256 encryption algorithm After decryption, the result data will be as follows: Random data (4 bytes).
ENCRYPTION_TYPE_IDTECH - Static variable in class com.datecs.api.emsr.EMSR
  Encrypted Magnetic Head IDTECH encryption algorithm, please refer to IDTECH documentation for detailed format and examples.
ENCRYPTION_TYPE_OLD_RSA - Static variable in class com.datecs.api.emsr.EMSR
  Card data will be sent encrypted in the format: Encryption type (1 byte): 01 - RSA2048 encrypted.
ENCRYPTION_TYPE_RSA - Static variable in class com.datecs.api.emsr.EMSR
  Card data will be sent encrypted in the format: Encryption type (1 byte): 01 - RSA2048 encrypted.
enrolIdentity(byte[]) - Method in class com.datecs.api.biometric.TouchChip
  Enrol finger print template in the TouchChip module non-volatile memory.
enrolIdentity(String) - Method in class com.datecs.api.biometric.TouchChip
  Enrol finger print template in the TouchChip module non-volatile memory.
ERROR_0K - Static variable in class com.datecs.api.universalreader.UniversalReader
  Operation successful.
ERROR_BARCODE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Barcode reader communication error.
ERROR_BARCODE_INVALID - Static variable in class com.datecs.api.universalreader.UniversalReader
  Barcode reader invalid command.
ERROR_BARCODE_NODATA - Static variable in class com.datecs.api.universalreader.UniversalReader
  No barcode read.
ERROR_BARCODE_NOTPRESENT - Static variable in class com.datecs.api.universalreader.UniversalReader
  Barcode reader not present.
ERROR_CARD - Static variable in class com.datecs.api.universalreader.UniversalReader
  Card error.
ERROR_FAILED - Static variable in exception com.datecs.api.rfid.RFIDException
  Command failed.
ERROR_INVALID - Static variable in class com.datecs.api.universalreader.UniversalReader
  Invalid command code.
ERROR_MIFARE_ACCESS - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare access error.
ERROR_MIFARE_AUTHENTICATION - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare authentication error.
ERROR_MIFARE_BIT - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare bit count error.
ERROR_MIFARE_CODE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare code error.
ERROR_MIFARE_COLLISION - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare collision error.
ERROR_MIFARE_CRC - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare CRC error.
ERROR_MIFARE_EACCESS - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare access error.
ERROR_MIFARE_EAUTHENTICATION - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare authentication error.
ERROR_MIFARE_EBASE - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare operation successful.
ERROR_MIFARE_EBIT - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare bit count error.
ERROR_MIFARE_ECODE - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare code error.
ERROR_MIFARE_ECOLLISION - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare collision error.
ERROR_MIFARE_ECRC - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare CRC error.
ERROR_MIFARE_EEEPROM - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare EEPROM error.
ERROR_MIFARE_EEPROM - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare EEPROM error.
ERROR_MIFARE_EFIFO - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare FIFO overflow.
ERROR_MIFARE_EFRAME - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare frame error.
ERROR_MIFARE_EGENERIC - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare generic error.
ERROR_MIFARE_EKEY - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare invalid key.
ERROR_MIFARE_EPARITY - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare parity error.
ERROR_MIFARE_ETIMEOUT - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare timeout error.
ERROR_MIFARE_EVALUE - Static variable in exception com.datecs.api.rfid.RFIDException
  Mifare value error.
ERROR_MIFARE_FIFO - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare FIFO overflow.
ERROR_MIFARE_FRAME - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare frame error.
ERROR_MIFARE_GENERIC - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare generic error.
ERROR_MIFARE_KEY - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare invalid key.
ERROR_MIFARE_PARITY - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare parity error.
ERROR_MIFARE_TIMEOUT - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare timeout error.
ERROR_MIFARE_VALUE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare value error.
ERROR_NODATA - Static variable in class com.datecs.api.universalreader.UniversalReader
  No data available.
ERROR_NORESPONCE - Static variable in class com.datecs.api.universalreader.UniversalReader
  No response from device.
ERROR_NOTPERMITTED - Static variable in class com.datecs.api.universalreader.UniversalReader
  Command not permitted.
ERROR_SYNTAX - Static variable in class com.datecs.api.universalreader.UniversalReader
  Syntax error.
ERROR_TIMEOUT - Static variable in exception com.datecs.api.rfid.RFIDException
  Timeout expired.
EVENT_NONE - Static variable in class com.datecs.api.hub.HUB
EVENT_SERIAL_PORT_RECV - Static variable in class com.datecs.api.hub.HUB
EVENT_USB_RECV - Static variable in class com.datecs.api.hub.HUB

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W