Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W

## C

calibrateBMMSensor() - Method in class com.datecs.api.printer.Printer
  Black mark mode sensor calibration.
CAPABILITY_BARCODE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Barcode reader capability.
CAPABILITY_BUTTON - Static variable in class com.datecs.api.universalreader.UniversalReader
  Button capability.
CAPABILITY_DEBUG - Static variable in class com.datecs.api.universalreader.UniversalReader
  Debug version capability.
CAPABILITY_EV15 - Static variable in class com.datecs.api.universalreader.UniversalReader
  Barcode reader EV15 capability.
CAPABILITY_FIRMWARE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Firmware download capability.
CAPABILITY_GSM - Static variable in class com.datecs.api.universalreader.UniversalReader
  GSM module capability.
CAPABILITY_LCD2X16 - Static variable in class com.datecs.api.universalreader.UniversalReader
  LCD 2x16 capability.
CAPABILITY_MAGNETIC - Static variable in class com.datecs.api.universalreader.UniversalReader
  Magnetic reader capability.
CAPABILITY_MIFARE - Static variable in class com.datecs.api.universalreader.UniversalReader
  Mifare reader capability.
CAPABILITY_SMARTCARD - Static variable in class com.datecs.api.universalreader.UniversalReader
  Smart card reader capability.
CAPABILITY_TOUCHSCREEN - Static variable in class com.datecs.api.universalreader.UniversalReader
  Touch screen capability.
capacity - Variable in class com.datecs.api.rfid.ContactlessCard
  The card capacity.
CARD_FELICA - Static variable in class com.datecs.api.rfid.ContactlessCard
  FeliCa
CARD_ISO14443A - Static variable in class com.datecs.api.rfid.ContactlessCard
  ISO 14443A.
CARD_ISO14443B - Static variable in class com.datecs.api.rfid.ContactlessCard
  ISO 14443B.
CARD_ISO15693 - Static variable in class com.datecs.api.rfid.ContactlessCard
  ISO 15693.
CARD_MIFARE_CLASSIC_1K - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Classic 1K.
CARD_MIFARE_CLASSIC_4K - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Classic 4K.
CARD_MIFARE_DESFIRE - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Desfire.
CARD_MIFARE_MINI - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Mini.
CARD_MIFARE_PLUS - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Plus.
CARD_MIFARE_ULTRALIGHT - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Ultralight.
CARD_MIFARE_ULTRALIGHT_C - Static variable in class com.datecs.api.rfid.ContactlessCard
  Mifare Ultralight C.
CARD_ST_SRI - Static variable in class com.datecs.api.rfid.ContactlessCard
  ST SRI
CARD_SUPPORT_FELICA - Static variable in class com.datecs.api.rfid.RFID
  FeliCa card.
CARD_SUPPORT_ISO15 - Static variable in class com.datecs.api.rfid.RFID
  ISO15 card.
CARD_SUPPORT_JEWEL - Static variable in class com.datecs.api.rfid.RFID
  JEWEL card.
CARD_SUPPORT_NFC - Static variable in class com.datecs.api.rfid.RFID
  NFC card.
CARD_SUPPORT_STSRI - Static variable in class com.datecs.api.rfid.RFID
  ST SRI card.
CARD_SUPPORT_TYPE_A - Static variable in class com.datecs.api.rfid.RFID
  TYPE A card.
CARD_SUPPORT_TYPE_B - Static variable in class com.datecs.api.rfid.RFID
  TYPE B card.
CARD_UNKNOWN - Static variable in class com.datecs.api.rfid.ContactlessCard
  Unknown card.
channel - Variable in class com.datecs.api.rfid.ContactlessCard
  The card channel.
CHANNEL_EMSR - Static variable in class com.datecs.api.printer.ProtocolAdapter
CHANNEL_FELICA - Static variable in class com.datecs.api.rfid.RC663
  FELICA channel.
CHANNEL_ISO1443A - Static variable in class com.datecs.api.rfid.RC663
  ISO1443A channel.
CHANNEL_ISO1443B - Static variable in class com.datecs.api.rfid.RC663
  ISO1443B channel.
CHANNEL_ISO15693 - Static variable in class com.datecs.api.rfid.RC663
  ISO15693 channel.
CHANNEL_MAIN - Static variable in class com.datecs.api.rfid.RC663
  Main channel.
CHANNEL_PRINTER - Static variable in class com.datecs.api.printer.ProtocolAdapter
  The channel associated with printer hardware module.
CHANNEL_RFID - Static variable in class com.datecs.api.printer.ProtocolAdapter
  The channel associated with RFID reader.
CHANNEL_STSRI - Static variable in class com.datecs.api.rfid.RC663
  ST SRI channel.
CHANNEL_UNIVERSAL_READER - Static variable in class com.datecs.api.printer.ProtocolAdapter
  The channel associated with Universal Reader hardware module.
checkIdentity() - Method in class com.datecs.api.biometric.TouchChip
  Check an identify.
close() - Method in class com.datecs.api.emsr.EMSR
  Close the streams and release all associated resources.
close() - Method in class com.datecs.api.hub.HUB
close() - Method in interface com.datecs.api.hub.SerialPort
close() - Method in class com.datecs.api.printer.Printer
  Close the streams and release all associated resources.
close() - Method in class com.datecs.api.printer.ProtocolAdapter.Channel
  Close channel.
close() - Method in class com.datecs.api.printer.ProtocolAdapter
  Close the streams and release all associated resources.
close() - Method in class com.datecs.api.rfid.RFID
  Close attached streams and release associated resources.
close() - Method in class com.datecs.api.universalreader.UniversalReader
  Close the streams and release all associated resources.
com.datecs.api - package com.datecs.api
com.datecs.api.biometric - package com.datecs.api.biometric
com.datecs.api.card - package com.datecs.api.card
com.datecs.api.emsr - package com.datecs.api.emsr
com.datecs.api.hub - package com.datecs.api.hub
com.datecs.api.printer - package com.datecs.api.printer
com.datecs.api.rfid - package com.datecs.api.rfid
com.datecs.api.smartcard - package com.datecs.api.smartcard
com.datecs.api.universalreader - package com.datecs.api.universalreader
completion() - Method in class com.datecs.api.rfid.STSRICard
  Card completion.
config() - Method in class com.datecs.api.universalreader.UniversalReader.MifareReader
  Configures Mifare card reader.
ContactlessCard - Class in com.datecs.api.rfid
  This class represents basic functionality of contactless card.
ContactlessCard(RC663) - Constructor for class com.datecs.api.rfid.ContactlessCard
  Create a new instance of this class.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W